{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["3.1 E.1 分部分项工程量清单计价表"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"3.1 E.1 分部分项工程量清单计价表","index":0,"n_rows":72,"n_cols":7,"rows_kept":72,"merged":[[0,0,0,6],[1,0,1,2],[1,5,1,6],[5,2,5,6],[8,0,10,0],[8,1,10,1],[8,3,10,3],[8,4,10,4],[8,5,10,5],[8,6,10,6],[12,0,14,0],[12,1,14,1],[12,3,14,3],[12,4,14,4],[12,5,14,5],[12,6,14,6],[16,0,18,0],[16,1,18,1],[16,3,18,3],[16,4,18,4],[16,5,18,5],[16,6,18,6],[20,0,22,0],[20,1,22,1],[20,3,22,3],[20,4,22,4],[20,5,22,5],[20,6,22,6],[23,2,23,6],[25,0,26,0],[25,1,26,1],[25,3,26,3],[25,4,26,4],[25,5,26,5],[25,6,26,6],[28,0,29,0],[28,1,29,1],[28,3,29,3],[28,4,29,4],[28,5,29,5],[28,6,29,6],[31,0,32,0],[31,1,32,1],[31,3,32,3],[31,4,32,4],[31,5,32,5],[31,6,32,6],[35,0,36,0],[35,1,36,1],[35,3,36,3],[35,4,36,4],[35,5,36,5],[35,6,36,6],[37,2,37,6],[54,2,54,6],[57,2,57,6],[68,0,69,0],[68,1,69,1],[68,3,69,3],[68,4,69,4],[68,5,69,5],[68,6,69,6],[71,0,72,0],[71,1,72,1],[71,2,72,2],[71,3,72,6]],"flags":["formulas_cached_only"]}
["E.1 分部分项工程量清单计价表"]
["工程名称：中共安徽省委党校（安徽行政学院）西校区专家楼装修改造工程项目",null,null,"标段：",null,"第1页 共1页"]
["序号","项目名称","项目特征","单位","数量","综合单价","合计"]
["一","1:专家楼仿古窗维修","专家楼整栋仿古窗维修：1破坏玻璃更换；2没有窗扇的补齐；3仿古窗木衬原油漆用砂纸抹平，调和漆刷两遍。投标单位自行查看现场，中标后不予调整。","项",1]
[null,"2:专家楼整体房间门窗维修","专家楼整体房间门窗维修：1维修掉拐；2坏的门锁更换；坏的玻璃更换；3门心缝用油灰添堵；4砂纸打磨，调和漆刷两遍。投标单位自行查看现场，中标后不予调整。","项",1]
[null,"小计"]
["二","吊顶"]
[null,"二楼会议室原吊顶拆除","二楼会议室吊顶拆除","M2",45]
[null,"二楼会议室吊顶安装-","二楼会议室吊顶安装:600mm×600mm铝扣扳吊顶","M2",45]
[null,null,"安装吊筋用φ8mm成品吊筋，打眼固定吊点间距为合理位置"]
[null,null,"安装主龙骨，主龙骨为烤漆38主龙骨，次龙骨为配套烤漆T型龙骨，龙骨基础水平件要调理平整，L型边条安装要用防锈自攻螺固定在墙面上，边条与墙面需弹线调至平行"]
[null,"北过道三楼吊顶拆除","北过道三楼吊顶拆除木板条1.75*36=63m2","M2",63]
[null,"北过道三楼吊顶","北过道吊顶安装:600mm×600mm铝扣扳吊顶","M2",63]
[null,null,"安装吊筋用φ8mm成品吊筋，打眼固定吊点间距为合理位置"]
[null,null,"安装主龙骨，主龙骨为烤漆38主龙骨，次龙骨为配套烤漆T型龙骨，龙骨基础水平件要调理平整，L型边条安装要用防锈自攻螺固定在墙面上，边条与墙面需弹线调至平行1.75*36*3（层）=189m2"]
[null,"南过道三楼吊顶拆除","南过道三楼吊顶拆除木板条1.75*36=63m2","M2",63]
[null,"南过道吊顶安装","南过道吊顶安装:600mm×600mm铝扣扳吊顶","M2",63]
[null,null,"安装吊筋用φ8mm成品吊筋，打眼固定吊点间距为合理位置"]
[null,null,"安装主龙骨，主龙骨为烤漆38主龙骨，次龙骨为配套烤漆T型龙骨，龙骨基础水平件要调理平整，L型边条安装要用防锈自攻螺固定在墙面上，边条与墙面需弹线调至平行1.75*36*3（层）=189m2"]
[null,"专家楼房间吊顶拆除","专家楼房间原扣板吊顶拆除及木龙骨拆除，三楼9个房间，二楼5间，一楼1间,共计15间","项",1]
[null,"专家楼房间吊顶","专家楼房间安装吊顶:600mm×600mm铝扣扳吊顶","M2",456]
[null,null,"安装吊筋用φ8mm成品吊筋，打眼固定吊点间距为合理位置"]
[null,null,"安装主龙骨，主龙骨为烤漆38主龙骨，次龙骨为配套烤漆T型龙骨，龙骨基础水平件要调理平整，L型边条安装要用防锈自攻螺固定在墙面上，边条与墙面需弹线平行，房间计：7.6m*4m=30.4m2。三楼9个房间，二楼5间，一楼1间,共计15间。30.4*15=456m2"]
[null,"小计"]
["三","乳胶漆（二楼会议室）铲除","墙面铲除至水泥沙浆层、墙面","M2",50]
[null,"乳胶漆（二楼会议室）","专家楼二楼墙面用沙纸打磨平整后植一遍胶","M2",50]
[null,null,"批二遍内墙腻子粉、用沙纸打磨平刷二遍内墙乳胶漆墙面。"]
[null,"北过道原乳胶漆铲除","墙面铲除至水泥沙浆层，北过道北面1.3*36*3层=140.4平米，北过道南墙面34*3.2*3层=326.4平米，合计140.4+326.4=460.8平米","M2",460.8]
[null,"北过道乳胶漆","专家楼北过道乳胶漆墙面用沙纸打磨平整后植一遍胶","M2",460.8]
[null,null,"批二遍内墙腻子粉、用沙纸打磨平刷二遍内墙乳胶漆墙面北过道北面1.3*36*3层=140.4平米，北过道南墙面34*3.2*3层=326.4平米，合计140.4+326.4=460.8平米"]
[null,"南过道北面原乳胶漆铲除","墙面铲除至水泥沙浆层，南过道北面墙40*3.4*3=408m2","M2",408]
[null,"南过道北面做外墙乳胶漆","专家楼南过道北面外墙乳胶漆墙面用沙纸打磨平整后植一遍胶","M2",408]
[null,null,"批二遍内墙腻子粉、用沙纸打磨平刷二遍内墙乳胶漆墙面北过道北面40*3.4*3=408m2"]
[null,"房间乳胶漆局部维修","专家楼房间原乳胶漆发霉及起壳处，铲除植胶一遍，批二遍内墙腻子粉、用沙纸打磨平刷二遍内墙乳胶漆（整体不能保证没有色差质量）","项",1]
[null,"楼梯原乳胶漆铲除","楼梯铲除至水泥沙浆层，墙面面积（8+3）*2*3.6高*3层=237.6；顶部面积8*3*3层=72合计237.6+72=309.6平米，加上一楼南进户厅墙面积顶部面积（7.6+4）2*3.6+7.6*4=112.48","M2",422]
[null,"楼梯乳胶漆做内墙乳胶漆","专家楼楼梯做乳胶漆墙面用沙纸打磨平整后植一遍胶","M2",422]
[null,null,"批二遍内墙腻子粉、刷二遍内墙乳胶漆,墙面面积（8+3）*2*3.6高*3层=237.6；顶部面积8*3*3层=72合计237.6+72=309.6平米，加上一楼南进户厅墙面积顶部面积（7.6+4）2*3.6+7.6*4=112.48"]
[null,"小计"]
["四","电器"]
[null,"总配电箱","总配电箱安装规格：500mm*600mm配电箱，内含100A漏保一个","套",1]
[null,"分户箱","每间安装pZ30箱，内含32A漏保一个，16A单匹两个，10A单匹1个（含楼会议室）","套",29]
[null,"电线","每层主电线16mm2，180米，共三层，180*3=540m（含会议室）","m",540]
[null,null,"进户线6mm2电线，每间9m,共9*10*3=270m（含会议室）","m",270]
[null,null,"每间空调线为4mm2每间30米,30*10*3=810m（含楼会议室）","m",810]
[null,null,"每间插座线2.5mm2,每间87米，87*10*3=2610m（含楼会议室）","m",2610]
[null,null,"照明电线1.5mm,每间30米，30*10*3=900m（含会议室）","m",900]
[null,"电线管","每间吊顶上电线用绝缘阻燃20PVC，30m*10*3（含会议室）","m",900]
[null,"明盒","每间安装明盒8个，8*10*3=240（含会议室）","个",240]
[null,"插座","每间安装16A空调插座一个，1*10*3=30（含会议室）","个",30]
[null,null,"每间安装地插3个10A,3*10*3=90（含会议室）","个",90]
[null,null,"每间安装开关单联单控2个，2*10*3=60（含会议室）","个",60]
[null,"灯","15间安装LED平板（含会议室）600*600灯两个，2*10*3","套",36]
[null,null,"北过道灯每层共5个，10*3=30","套",15]
[null,null,"楼梯安装吸顶灯","套",6]
[null,"小计"]
["五","高空作业脚手架",null,"项",1]
["六","垃圾清理及外运费",null,"项",5000]
["七","清单费"]
["八","项目名称（卫生间改造）","项目特征","单位","数量","综合单价","合计"]
["九","拆除","拆除卫生间地砖至基层及排水铸铁管道","项",1]
["十","防水","卫生间地面找平后做JS或丙纶防水，两遍.","间",15]
["十一","下水管道","卫生间做下水管道，主管PVC110,支管PVC50.吊卡支撑固定下水管道，符合规范要求。","间",15]
["十二","铺设地砖","卫生间地砖铺设，300*300地砖，每个卫生间5.5平米5.5*5*3=82.5","M2",82.5]
["十三","安装坐便器","每个卫生间安装坐便器一个（含辅材）1*5*3=15","套",15]
["十四","安装拖把池","每个卫生间安装拖把池一个（含辅材）1*5*3=15","套",15]
["十五","安装洗脸盆","每个卫生间安装洗面盆一个（含辅材）1*5*3=15","套",15]
["十六","地漏","每个卫生间安装不锈钢防臭地漏一个（含辅材）1*5*3=15","套",15]
["十七","卫生间原乳胶漆铲除","卫生间原乳胶漆铲除至水泥沙浆层，墙面面积为；（2.5+2.2）*2*1.9高*5间*3层=267.9平米","M2",267.9]
["十八","卫生间做内墙乳胶漆","专家楼卫生间做乳胶漆墙面用沙纸打磨平整后植一遍胶","M2",267.9]
[null,null,"批二遍内墙腻子粉、刷二遍内墙乳胶漆墙面面积为；（2.5+2.2）*2*1.9高*5间*3层=267.9平米"]
["小计"]
["二十"," 含税合计"]