{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["参数"],"not_rendered":{"images":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"参数","index":0,"n_rows":5,"n_cols":8,"rows_kept":5,"merged":[[0,0,0,7],[2,0,3,0],[4,1,4,7]],"flags":["formulas_cached_only"]}
["考勤机参数"]
["系统","名称","规格型号","产地品牌","单位","数量","参数","    图片"]
["广域网考勤机","人脸考勤机(含BS考勤模块）","iface702","ZKTeco","台",30,"RS492TCP/IP、USB-host，用户(卡)容量：1万枚；指纹容量：2000枚；面部容量：500张；19万条，功能特性：记录查询、Photo ID、TTS语音播报、定时响铃、多种验证方式、T9输入法、天气预报、简单门禁、Wiegand Out、外接响铃、带摄像头 、联网考勤信息自动上传软件。"]
[null,"ZKTime10.0BS考勤软件","50点位","ZKTeco","台",1,"    ZKTime10.0使用世界流行的Apache作为WEB服务，并采用特殊技术实时监控服务的运行，确保了永不死机，完全能满足各种规模企业的考勤应用，尤其超大型企业优势表现更为明显，由于使用Apache服务，因而可以方便采用代理、集群等技术，使系统无限扩展。\n      ZKTime10.0系统平台以“身份识别技术”为核心，包括刷卡、指纹、面部、静脉、掌纹等，整合了互联网应用三大核心要素：计算、存储、网络，通过创新的设计，将时间与安全有机的结合，最终实现单位的精细化管理。\n数据自动上传下载，实现真正无人值守， 数据可加密、压缩传送"]
["备注","硬件设备免费保修一年，保修期外，只收取硬件成本费用，公司终身提供维修服务。产品维修一般通过送修、电话报修、网上报修、上门维修等形式来完成，维修迅速、及时。提供在现场维修设备以至正常运行服务，并使用户能正确使用。软件设备免费保修一年，保修期外只收取上门费，软件永久质保。"]