{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":16,"n_cols":7,"rows_kept":16,"merged":[[0,0,0,6],[3,0,4,0],[3,1,4,1],[3,6,4,6],[5,0,7,0],[5,1,7,1],[5,6,7,6],[8,0,10,0],[8,1,10,1],[8,6,9,6],[13,1,13,2],[14,1,14,2],[15,0,15,6]],"flags":["formulas_cached_only"]}
["西校区部分地块整治工程项目工程量清单"]
["序号","工　作　内　容","规格及要求","单位","数量","金额","备注"]
[1,"沿望江路边栽植两排夹竹桃（130米）","苗高180cm；冠幅80cm；4株/m","株",520,null,"养护期一年"]
[2,"二马路东地块破除挡土墙并平整","破除挡土墙并平整（垃圾外运）","M2",2100]
[null,null,"清理杂树","项",1]
[3,"二马路东铺道板砖","铺设红黄双色方砖，规格：25*25cm","M2",43]
[null,null,"铺道板砖混凝土基层，厚度10cm","M2",43]
[null,null,"铺装侧石，材质：大理石；规格：长100cm厚12cm高20cm","M",67.2]
[4,"填土并做暗排水渠","拉土方的车费及装卸等机械费用","M3",1400,null,"土方由本校内提取"]
[null,null,"土方平整费用(根据现场业主要求，形成自然坡度）","M2",2900]
[null,null,"做排水井和暗排水管道（井口80*80，深1.5M；预埋管道规格：Φ50cm，长度：1000cm，材质：塑料波纹管）","项",1,null,"暂定"]
[5,"场地细整","铺草坪前人工细整","M2",2900]
[6,"马尼拉","满铺","M2",2900,null,"养护期一年"]
[7,"税金（10%）"]
[8,"总计"]
["备注：绿化部分养护期为一年"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}